# AudioScience Dante Iyo firmware

Table of Contents

- Known Issues
- Releases
  - Build v3.5.8 (January 2022)
  - Build v3.5.7 (December 2021)
  - Build v3.5.6 (December 2021)
  - Build v3.5.5 (December 2021)
  - Build v3.5.4 (December 2021)
  - Build v3.5.3 (October 2021)
  - Build v3.4.2 (September 2021)
  - Build v3.4.0 (October 2020)
  - Build v3.3.1 (March 2020)
  - Build v3.3.0 (March 2020)
  - Build v3.2.3 (January 2020)
  - Build v3.2.2 (January 2020)
  - Build v3.2.1 (December 2019)
  - Build v3.2.0 (November 2019)
  - Build v3.1.0 (August 2019)
  - Build v3.0.0 (July 2019)
  - Build v2.2.2 (June 2019)
  - Build v2.2.1 (May 2019)
  - Build v2.2.0 (March 2019)
  - Build v2.1.1 (March 2019)
  - Build v2.1.0 (February 2019)
  - Build v2.0.1 (January 2019)
  - Build v2.0.0 (January 2019)
  - Build v1.1.0 (December 2018)
  - Build v1.0.5 (December 2018)
  - Build v1.0.4 (December 2018)
  - Build v1.0.3 (November 2018)
  - Build v1.0.2 (November 2018)
  - Build v1.0.1 (October 2018)

# Known Issues

# Releases

## Build v3.5.8 (January 2022)

- build changes: upload directory path and creates zip of output files

## Build v3.5.7 (December 2021)

- wasp: set password to disabled by default

## Build v3.5.6 (December 2021)

- same as 3.5.5 but disabled io count test (hanging Travis)

## Build v3.5.5 (December 2021)

- same as 3.5.4 but built on master branch

## Build v3.5.4 (December 2021)

- note: not built on master branch
- asi27xx: enable ui password with disable

## Build v3.5.3 (October 2021)

- oem: add support for OEM serial number
- misc: bugfixes

## Build v3.4.2 (September 2021)

- hwio: reduce unmute delay to 100ms after toggling phantom

## Build v3.4.0 (October 2020)

- wasp: update WASP conf files to WASP version 3.2.0
- wasp: support X-Wasp-Stream-Min-Update-Period and X-Wasp-Stream-Exclude-Obj-Type headers

## Build v3.3.1 (March 2020)

- dante: fix Dante device prefix names for some models

## Build v3.3.0 (March 2020)

- dante: support 88.2kHz sample rate
- audinate: update brooklyn II firmware from 4.0.9.1 to 4.2.0.28
- UI: flash meter LED red when phantom is on; cycle between red and blue when both phantom and mute are on
- UI: always cycle through the complete identify LED identify sequence

## Build v3.2.3 (January 2020)

- oem: add support for ASI2791: 4x mic in, 8x line in -> 12x mic/line in

## Build v3.2.2 (January 2020)

- py lw: further bug fixes for Pathfinder PC/Pro

## Build v3.2.1 (December 2019)

- py lw: fixes for Pathfinder PC/Pro

## Build v3.2.0 (November 2019)

- py lw: implement Livewire GPIO

## Build v3.1.0 (August 2019)

- webui: add GPIO interface (RJ-45 models)
- webui: modify AES67 interface to allow specific transport IP addresses
- py lw: advertisement bugfix

## Build v3.0.0 (July 2019)

- WASP 3.0 (http://www.audioscience.com/internet/download/sdk/wasp/wasp_3.0.0.html)
- support for 14 new DB25 and RJ45 connector models
- AES67 interface UI changes

## Build v2.2.2 (June 2019)

- wasp: implement bulk patch support as spcified in version 2.1.0

## Build v2.2.1 (May 2019)

- webui: remove non-applicable menu options from Input only and Output models

## Build v2.2.0 (March 2019)

- hwio/webui: add output mute
- conf: added OEM configuration

## Build v2.1.1 (March 2019)

- hwio: keep SYS led orange until objects restore is complete

## Build v2.1.0 (February 2019)

- hwio: cycle input meter LEDs blue when muted
- py: unit test fixes (e.g. property validation)

## Build v2.0.1 (January 2019)

- py: HTTP server fixes

## Build v2.0.0 (January 2019)

- WASP 2.0: publish specification (http://www.audioscience.com/internet/download/sdk/wasp/wasp_2.0.9.html)
- py: support bulk PATCH methods
- web-ui: improved performance

## Build v1.1.0 (December 2018)

- web-ui: add Mute button

## Build v1.0.5 (December 2018)

- config: define Product Version

## Build v1.0.4 (December 2018)

- hwio/web-ui: add temperature sensor

## Build v1.0.3 (November 2018)

- hwio: bug fix for mic pre levels +5 to +10 dBu

## Build v1.0.2 (November 2018)

- web-ui: display gain in dB instead of level in dBu on inputs
- http: support method overriding
- hwio/web-ui: bypass pad on input levels of 0 to +10dBu
- web-ui: add Settings tab with LED Brightness option
- models: add ASI2705, ASI2706, ASI2708, ASI2709 (16.0M, 32.0M, 0.16L, 0.32L)
- web-ui: disable phantom power button when pad is engaged
- web-ui: add AES67 streaming feature

## Build v1.0.1 (October 2018)

- First release build